# PCASM

Use the (restricted) additive Schwarz method, each block is (approximately) solved with its own KSP object.

### Options Database Keys

| -pc_asm_truelocal | - Activates PCASMSetUseTrueLocal()
| -pc_asm_in_place | - Activates in-place factorization
| -pc_asm_blocks <blks> | - Sets total blocks
| -pc_asm_overlap <ovl> | - Sets overlap
| -pc_asm_type [basic,restrict,interpolate,none] | - Sets ASM type

IMPORTANT: If you run with, for example, 3 blocks on 1 processor or 3 blocks on 3 processors you will get a different convergence rate due to the default option of -pc_asm_type restrict. Use -pc_asm_type basic to use the standard ASM.

Notes: Each processor can have one or more blocks, but a block cannot be shared by more than one processor. Defaults to one block per processor.

To set options on the solvers for each block append -sub_ to all the KSP, and PC options database keys. For example, -sub_pc_type ilu -sub_pc_ilu_levels 1 -sub_ksp_type preonly

To set the options on the solvers seperate for each block call PCASMGetSubKSP() and set the options directly on the resulting KSP object (you can access its PC with KSPGetPC())

### See Also

PCCreate(), PCSetType(), PCType (for list of available types), PC,
PCBJACOBI, PCASMSetUseTrueLocal(), PCASMGetSubKSP(), PCASMSetLocalSubdomains(), PCASMSetTotalSubdomains(), PCSetModifySubmatrices(), PCASMSetOverlap(), PCASMSetType(), PCASMSetUseInPlace()

Level:beginner
Location:src/ksp/pc/impls/asm/asm.c
Index of all PC routines
Table of Contents for all manual pages
Index of all manual pages

### Examples

src/ksp/examples/tutorials/ex8.c.html